Documentation: NexRadio.h Source File

| Documentation For Arduino users

- Main Page
- Related Pages
- Modules
- Classes
- Files
- Examples

- File List
- File Members

NexRadio.h
Go to the documentation of this file.
1
17 #ifndef __NEXRADIO_H__
18 #define __NEXRADIO_H__
19
20 #include "NexTouch.h"
21 #include "NexHardware.h"
35 class NexRadio:public NexTouch
36 {
37 public: /* methods */
38
42 NexRadio(uint8_t pid, uint8_t cid, const char *name);
43
50 uint32_t getValue(uint32_t *number);
51
58 bool setValue(uint32_t number);
59
66 uint32_t Get_background_color_bco(uint32_t *number);
67
74 bool Set_background_color_bco(uint32_t number);
75
82 uint32_t Get_font_color_pco(uint32_t *number);
83
90 bool Set_font_color_pco(uint32_t number);
91
92 };
98 #endif /* #ifndef __NEXRADION_H__ */
NexRadio::Get_background_color_bco
uint32_t Get_background_color_bco(uint32_t *number)
Get bco attribute of component.
Definition: NexRadio.cpp:45
NexRadio::Get_font_color_pco
uint32_t Get_font_color_pco(uint32_t *number)
Get pco attribute of component.
Definition: NexRadio.cpp:73
NexRadio
NexRadio component.
Definition: NexRadio.h:35
NexRadio::setValue
bool setValue(uint32_t number)
Set val attribute of component.
Definition: NexRadio.cpp:31
NexRadio::getValue
uint32_t getValue(uint32_t *number)
Get val attribute of component.
Definition: NexRadio.cpp:22
NexTouch.h
The definition of class NexTouch.
NexHardware.h
The definition of base API for using Nextion.
NexRadio::Set_background_color_bco
bool Set_background_color_bco(uint32_t number)
Set bco attribute of component.
Definition: NexRadio.cpp:55
NexRadio::Set_font_color_pco
bool Set_font_color_pco(uint32_t number)
Set pco attribute of component.
Definition: NexRadio.cpp:83
NexTouch
Father class of the components with touch events.
Definition: NexTouch.h:53
NexRadio::NexRadio
NexRadio(uint8_t pid, uint8_t cid, const char *name)
Constructor.
Definition: NexRadio.cpp:17