Documentation: NexCrop.h Source File

| Documentation For Arduino users

- Main Page
- Related Pages
- Modules
- Classes
- Files
- Examples

- File List
- File Members

NexCrop.h
Go to the documentation of this file.
1
17 #ifndef __NEXCROP_H__
18 #define __NEXCROP_H__
19
20 #include "NexTouch.h"
21 #include "NexHardware.h"
30 class NexCrop: public NexTouch
31 {
32 public: /* methods */
33
37 NexCrop(uint8_t pid, uint8_t cid, const char *name);
38
47 bool Get_background_crop_picc(uint32_t *number);
48
57 bool Set_background_crop_picc(uint32_t number);
58
67 bool getPic(uint32_t *number);
68
77 bool setPic(uint32_t number);
78 };
79
84 #endif /* #ifndef __NEXCROP_H__ */
NexCrop::Get_background_crop_picc
bool Get_background_crop_picc(uint32_t *number)
Get the number of picture.
Definition: NexCrop.cpp:23
NexCrop::getPic
bool getPic(uint32_t *number)
Get the number of picture.
Definition: NexCrop.cpp:46
NexCrop::NexCrop
NexCrop(uint8_t pid, uint8_t cid, const char *name)
Constructor.
Definition: NexCrop.cpp:18
NexTouch.h
The definition of class NexTouch.
NexHardware.h
The definition of base API for using Nextion.
NexCrop::setPic
bool setPic(uint32_t number)
Set the number of picture.
Definition: NexCrop.cpp:55
NexCrop
NexCrop component.
Definition: NexCrop.h:30
NexCrop::Set_background_crop_picc
bool Set_background_crop_picc(uint32_t number)
Set the number of picture.
Definition: NexCrop.cpp:32
NexTouch
Father class of the components with touch events.
Definition: NexTouch.h:53