Documentation: CompGauge.ino

| Documentation For Arduino users

- Main Page
- Related Pages
- Modules
- Classes
- Files
- Examples

CompGauge.ino

How to Use
  This example shows that ,when the "btn_up" component on the Nextion screen is released, the value of gauge component will plus 5, when the "btn_down" component released, the value of gauge component will minus 5 every time.

Author
  Wu Pengfei (email:pengf.nosp@m.ei.w.nosp@m.u@ite.nosp@m.ad.c.nosp@m.c)

Date
  2015/7/10 2016/12/25 bring HMI up to v0.32 to avoid too old issues by Patrick Martin, no other changes made

Copyright
  Copyright (C) 2014-2015 ITEAD Intelligent Systems Co., Ltd.
  This program is free software; you can redistribute it and/or modify it under the terms of the GNU General Public License as published by the Free Software Foundation; either version 2 of the License, or (at your option) any later version.